पत्र सं0 23( 16 ) @सि मा अनु परिमं एम**&**31/2130 दिनांक 10.06.15

**Inspection Note**

The work of repair of footpath of Chhatra Marg, Delhi University area, was inspected on 09.06.2015. The repair work is being done to make the footpath disabled friendly and to take care of the observations made by the PWD appointed Consultant for Access Audit of Delhi University roads. The following directions were issued were noted for compliance by the contractor and the Executive Engineer.

1 Although old red sand stone was being reused in the portion of footpath inspected, but it was directed that only the stones with sharp and square edges be used and broken / rugged edged stones should be discarded. The pattern / design, as was existing before dismantling of the footpath, should be maintained.

2 The openings being left for manholes over the underlying drain should have mild steel angle frame. The top edge of the MS angle should be flush with the finished level of the stone pavement.

3 The ramps presently provided in front of the gates should now be modified and developed as table-tops in such a way that major portion is horizontal and level with the footpath so that there is minimum inconvenience to the pedestrians.

4 RCC bollards should be provided at the junction of footpaths and ramps / table tops provided in front of the gates. Similarly warning / dotted paver blocks should be provided at the end of footpath but before the bollards.

5 It is expected that 70-80% of existing red sand stone shall be reused in footpath repair. However, new red sand stone should be provided in a separate patch at the end and should not be intermixed with the existing / old red sand stone.

6 The signages should be raised so that the bottom level of board is atleast 2.1m above the finished footpath level. The junction of signage pole with footpath should be neatly finished.

**Page 1 of 2**

7 The work should be finished within 10 days’ time.

**अधीक्षण अभियंता**

**सि मा अनु परि एम 31**

**पंजाबी बाग नई दिल्ली**

**प्रतिलिपि -**

1 The Chief Engineer, PWD M-3, MSO Building, New Delhi

2 OSD to Hon’ble Minister (PWD), 7th Floor, Delhi Sectt., New Delhi – 110 002.

3 The Executive Engineer, CRMD M-313, Opposite Khalsa College, Mall Road, Delhi

4 Guard File

**अधीक्षण अभियंता**